**Comment/Explanation\*:***Include your justification for your proposed change to the draft standard below.*  
\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Under Section A-1.4.1 General Installation Requirements for FPIS, the formatting of the subsection needs to be corrected to remove the double indent for Sections currently marked as A-1.4.1.2.1 and A-1.4.1.3. The correct section numbers are listed below.

**Proposed Change to the Draft Standard\***  
*Use “strikethrough” and “underline” formatting to indicate all proposed changes. Changes must be shown with “hard-formatting” strikethrough and underline, not “track changes”.*

*Use a color other than red to indicate proposed changes to the draft.*\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Correct formatting so the section numbers under A-1.4.1 appear as follows:

A-1.4.1.1 FPIS shall be installed on the interior…

A-1.4.1.2 FPIS shall be installed without gaps…

A-1.4.1.3 When FPIS is installed in multiple layers….

A-1.4.1.4 FPIS shall be installed in contact…

A-1.4.1.5 Damage to FPIS during installation…

A-1.4.1.6 When specified as a radient barrier…