**Comment/Explanation\*:***Include your justification for your proposed change to the draft standard below.*
\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

(Pg. 12)

**4.1.1 Projected Assessments** are generated prior to construction wherein the actual installed conditions, equipment, and systems are not yet completed or installed. *Projected Assessments* shall be conducted in accordance with Sections 5, 6 and 7.

4.1.1.1 All *Minimum Assessed Products* for a *Projected Assessment* shall be determined from *construction documents* for a new or existing home in accordance with Tables 10.1.1 and 10.1.5.

### **4.1.2 Confirmed Assessments** are conducted, generated, and verified after completion of construction in accordance with Sections 5, 6 and 7.

#### 4.1.2.1 All Minimum Assessed Products for a Confirmed Assessment shall be determined from construction documents and/or on-site measurements for new or existing homes in accordance with Table 5.4.1 and verified according to the requirements in Section 7.

Table 5.4.1 should be referenced under section *4.1.1.1 All Minimum Assessed Products for a Projected Assessment* as well as being referenced in section *4.1.2.1 All Minimum Assessed Products for a Confirmed Assessment.* Table 5.4.1 outlines minimum assessed products which are just as important in a projected rating as they are in a confirmed rating.

**Proposed Change to the Draft Standard\***
*Use “strikethrough” and “underline” formatting to indicate all proposed changes. Changes must be shown with “hard-formatting” strikethrough and underline, not “track changes”.*

*Use a color other than red to indicate proposed changes to the draft.*\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

4.1.1.1 All *Minimum Assessed Products* for a *Projected Assessment* shall be determined from *construction documents* for a new or existing home in accordance with Tables 5.4.1, 10.1.1 and 10.1.5.