**Comment/Explanation\*:***Include your justification for your proposed change to the draft standard below.*  
\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

We recommend removing the building components below from the Exclusions list. These building components have widely available LCA/EPD/PEP data and/or represent material impacts within a home. Additionally, consistent with our comment on the Foreword on page 4, we recommend that this list is reviewed annually for updating as more LCA/EPD data becomes available.

**Proposed Change to the Draft Standard\***  
*Use “strikethrough” and “underline” formatting to indicate all proposed changes. Changes must be shown with “hard-formatting” strikethrough and underline, not “track changes”.*

*Use a color other than red to indicate proposed changes to the draft.*\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

10.4 Building Components Exclusions (Informative)

The following building products are not required and shall not be included in an embodied carbon assessment for compliance with this Standard…

~~Soffit~~

~~Door hardware~~

~~Cabinetry~~

~~Counters~~

~~Light Fixtures~~

~~Solar/PV systems~~

~~Balconies, porches, decks, ramps~~